PEP-Version: 2.41
Active Prog-Express mode: Read
Connected Programmers: 0

;**************************************
 Mode: Program
;**************************************
 ; Destination chip settings:
    Destination chip variant id: %CHIPID%
    Destination chip name: %CHIPNAME%

 ; File dialog:
    FileName: 
    MultiFileMode: False
    Checksum Algorithm: Sum
    Further information: False

 ; Chip option settings:
    Split option: All
    Chip memory number: 0
    Memory used: True
    Real time clock option: NoChanges
    Real time clock date time: 09.03.2012 14:51:52
    Real time clock calibration: 0

 ; Serial number settings:
    Serial number mode: Off
    Serial number file: 
    Actual position: 1
    Chip address for the first serial byte: 0
    Number of serial number bytes: 8
    Next serial number: 0
    Serial number increment by: 1
    Endian: BigEndian
    Number base: Dec
    Number format: AsciiText

 ; Copies:
    Copies: 1

 ; Process jobs:
    Show jobs: False
    Process job (0): True
    Process job (1): True
    Process job (2): False
    Process job (3): True
    Process job (4): True
    Process job (5): True
    Process job (6): True
    Process job (7): False
    Process job (8): False
    Process job (9): True
    Process job (10): True
    Process job (11): True

;**************************************
 Mode: Copy
;**************************************

 ; Serial number settings:
    Serial number mode: Off
    Serial number file: 
    Actual position: 1
    Chip address for the first serial byte: 0
    Number of serial number bytes: 8
    Next serial number: 0
    Serial number increment by: 1
    Endian: BigEndian
    Number base: Dec
    Number format: AsciiText

 ; Copies:
    Copies: 1

 ; Process jobs:
    Show jobs: False
    Process job (0): True
    Process job (1): True
    Process job (2): True
    Process job (3): True
    Process job (4): True
    Process job (5): True
    Process job (6): True
    Process job (7): True
    Process job (8): True
    Process job (9): True
    Process job (10): True
    Process job (11): True

;**************************************
 Mode: Read
;**************************************
 ; Source chip settings:
    Source chip variant id: 697
    Source chip name: AM29F400BB

 ; File dialog:
    FileName: C:\Users\th\AppData\Local\Temp\tmp_54c80bb\dat.bin

 ; Chip option settings:
    Split option: All
    Chip memory number: 0
    Memory used: True
    Real time clock option: NoChanges
    Real time clock date time: 09.03.2012 14:51:52
    Real time clock calibration: 0

 ; Serial number settings:
    Serial number mode: Off
    Serial number file: 
    Actual position: 1
    Chip address for the first serial byte: 0
    Number of serial number bytes: 8
    Next serial number: 0
    Serial number increment by: 1
    Endian: BigEndian
    Number base: Dec
    Number format: AsciiText

 ; Copies:
    Copies: 1

 ; Process jobs:
    Show jobs: True
    Process job (0): True
    Process job (1): True
    Process job (2): True
    Process job (3): True
    Process job (4): True
    Process job (5): True
    Process job (6): True
    Process job (7): True
    Process job (8): True
    Process job (9): True
    Process job (10): True
    Process job (11): True

;**************************************
 Mode: Production
;**************************************
    MultiFileMode: False
    Checksum Algorithm: Sum
    Further information: False

 ; Chip option settings:
    Split option: All

 ; Serial number settings:
    Serial number mode: Off
    Serial number file: 
    Actual position: 1
    Chip address for the first serial byte: 0
    Number of serial number bytes: 8
    Next serial number: 0
    Serial number increment by: 1
    Endian: BigEndian
    Number base: Dec
    Number format: AsciiText

 ; Copies:
    Copies: 1

 ; Process jobs:
    Show jobs: False
    Process job (0): True
    Process job (1): True
    Process job (2): True
    Process job (3): True
    Process job (4): True
    Process job (5): True
    Process job (6): True
    Process job (7): True
    Process job (8): True
    Process job (9): True
    Process job (10): True
    Process job (11): True

;**************************************
; Specific programmer settings 
;**************************************
    Use programmer specified chip: False
    Use programmer specified file: False
    Use programmer specified chip options: False

;**************************************
 Mode: Hex-Editor
;**************************************
 ; Destination chip settings:
    Hex-Editor chip variant id: 697
    Hex-Editor chip name: AM29F400BB

 ; Open Files:
    Hex-Editor file: c:\users\th\desktop\delme.bin
    Hex-Editor file: c:\users\th\desktop\delme.bin
    Hex-Editor file: c:\users\th\desktop\delme.bin
 ; Chip option settings:
    Split option: All
    Chip memory number: 0
    Memory used: True
    Real time clock option: NoChanges
    Real time clock date time: 09.03.2012 14:51:52
    Real time clock calibration: 0

 ; Serial number settings:
    Serial number mode: Off
    Serial number file: 
    Actual position: 1
    Chip address for the first serial byte: 0
    Number of serial number bytes: 8
    Next serial number: 0
    Serial number increment by: 1
    Endian: BigEndian
    Number base: Dec
    Number format: AsciiText


;**************************************
; Global Programmer Settings
;**************************************
    Fill unused bytes with: 255
    Mirror Buffer: False
    Byte order: LittleEndian
    Verify voltage minimal: False
    Verify voltage nominal: True
    Verify voltage maximal: False
    Test pin contacts: True
    Overcurrent monitoring: True

;**************************************
; Operator Settings
;**************************************
    Lock is activated: False
    Lock mode selection: False
    Lock password used: False
    Lock password hash: 
